|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Getting started with your new BroodMinder beehive monitors  (more help at MyBroodMinder.com) |  | |  | A close up of a logo  Description automatically generated |
| BroodMinder-T2SM   1. Press button > 5 seconds 2. A picture containing text, electronics     Description automatically generated-T2SM will blink 15 seconds | | BroodMinder-TH2SM   1. Pull battery tab 2. -TH2SM will blink 15 seconds | BroodMinder-W   1. Pull battery tab 2. -W will blink 15 seconds | BroodMinder-W2   1. Pull battery tab 2. -W2 will flash 15 seconds |
| Install the -T2SM above the lower  brood box on the middle frames | | Install the -TH2SM above the upper  brood box on the middle frames | Install the -W under the hive with a  2x4 or angle pivot to make it level | Install the -W2 on the bottom board |

|  |  |  |  |
| --- | --- | --- | --- |
| **Create cloud apiary**   1. Create a MyBroodMinder.com account 2. Create virtual apiary 3. Create virtual hives | **Retrieve BroodMinder Data**   1. Load BroodMinder-apiary app 2. Enter username and password 3. Wait for device IDs to show on list 4. Tap device ID & sync data to cloud       Apiary app display | **Assign Devices**   1. Log into MyBroodMinder.com 2. Choose “Configure” 3. Choose “Devices” 4. Assign devices to hive location | **Analyze Data**   1. Log into MyBroodMinder.com 2. Choose “Mellisphera” 3. Choose “Explore” |

A close up of a logo

Description automatically generatedPrinting instructions:

This should be printed double sided and tri-folded so that

Is on the outside.

The width of the folded assembly must be 1.7” or slightly less because it must fit inside another assembly.